HV+(L) is connected to HV- (M), and HV+(M) is connected to HV-(R).HV connection for the 7-chip (z&f) hybridHV connection for the 5-chip (z&f) hybrid

HV(L) to sensor

Finger 7HV+(L)/HV-(R)

Jumper FieldHV(R)GHV+(R)HV(R)HV-(R)HV(R)HV(L)G0.0056mFHV+(L) is connected to HV-(R).

HV+(R)

HV(L) to sensor

Finger 5HV(L)GHV(L)HV-(L)HV+(L)HV(L)

Jumper FieldHV+(L)/HV-(M)HV(R)GHV+(R)HV(R)0WHV-(R)HV(R)HV+(R)

Jumper FieldHV(M)HV-(M)HV(M)GHV+(M)HV(M)0.0056mF

Jumper FieldHV+(L)/HV-(M)HV(L)HV-(L)HV+(L)HV(L)10K (f ONLY!)

Jumper Field0W10K0W(z ONLY!)0W(z ONLY!)0W(z ONLY!)0W(z ONLY!)10K(z ONLY!)Cable connected on left side.Cable is connected in the middle.