HV+(L) is connected to HV- (R).HV+(L)HV(L)HV(L)HV-(L)HV(L)G

HV(L) to sensor

Finger 1

Jumper FieldHV+(R)HV(R)HV(R)HV-(R)HV(R)G0W0W10K0.0056mFHV connection for the 4-chip (z) hybridHV connection for the 6-chip (f) hybrid

HV(L) to sensor

Finger 1HV+(L)/HV-(R)

Jumper FieldHV(R)GHV+(R)HV(R)HV(R)HV-(R)HV+(L)HV(L)10KHV(L)G0.0056mFHV-(L)HV(L)HV+(L) is connected to HV-(R).

HV+(L)/HV-(R)HV+(R), to jumperHV+(R), to jumper