Hybrid 2p18 Traveler

September 29, 1999

1 Connectivity

Repairs on shorts:

Fixes for opens:

added wire to fix Bus 7 open in cable

2 Chips

The following chips were assembled on this hybrid (in the order that the chips get read out):

Hybrid 2P18 has die: 078-045 078-048

3 Bad Channels

The following channels were bad or exceedingly noisy: Cell 9 is bad.

4 Comments

No comments.

5 Pedestal

The following plot shows the pedestals vs. channel number Pedestal

The following plot shows the average pedestal vs. pipeline cell ID. The x-axis is cell ID offset by 46 for each chip. Thus cell ID 5 on chip 1 ia at x=5, chip 2 at x=49, chip 3 at x=97, etc. Pedestal vs. Pipeline Cell ID

6 Noise

The following plot shows the single cell RMS noise: RMS Noise

The following plot show the multi-cell RMS noise: Multi-Cell Noise

7 Dynamic Threshold Subtraction

The following plot shows the readout of channels with charge injection with the dynamic threshold subtraction turned on: Dynamic Threshold Subtraction