Silicon Tracks See Beam Spot

• During 36x36 collisions in April, 2001, we had 2 wedges of silicon detector integrated as test of full system

• Able to measure position of interaction point

• Measurement confirmed by independent devices (COT, calorimeter)

Cluster Charge

• Silicon sensors in good working order. Cluster charges are Landau distributions.